"Source:"	"/media/jrc/SDA_D/Kicad/SBC-188v3/SBC-188v3.sch"
"Date:"	"Fri 21 Feb 2020 07:38:29 AM PST"
"Tool:"	"Eeschema 5.1.5-52549c5~84~ubuntu16.04.1"
"Component Count:"	"102"
"Ref"	"Value"	"Part"	"Footprint"	"Description"	"Vendor"
"C301"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C302"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C303"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C304"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C305"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C306"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C307"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C308"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C309"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C310"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C311"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C312"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C313"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C314"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C315"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C316"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C317"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C318"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C319"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C320"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C321"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C322"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C323"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C324"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C325"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C326"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C327"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C328"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C329"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C330"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C331"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C332"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C333"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C334"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C335"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C336"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C337"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C338"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C339"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C340"	"0.1"	"device:C"	"discret:C2"	"Condensateur non polarise"	""
"C341"	"47uf"	"device:CP"	"discret:C1V7"	"Condensateur polarise"	""
"C342"	"47uf"	"device:CP"	"discret:C1V7"	"Condensateur polarise"	""
"C343"	"47uf"	"device:CP"	"discret:C1V7"	"Condensateur polarise"	""
"C344"	"47uf"	"device:CP"	"discret:C1V7"	"Condensateur polarise"	""
"C601"	"10uF"	"device:CP"	"discret:C1V5"	"Condensateur polarise"	""
"C701"	"0.47F"	"device:CP"	"N8VEM:SuperCap5"	"Condensateur polarise"	""
"D601"	"LED"	"device:LED"	"N8VEM:LED-5MM-POL"	""	""
"D701"	"LED"	"01RetroBrew:LED"	"N8VEM:LED-5MM-POL"	""	""
"D702"	"LED"	"01RetroBrew:LED"	"N8VEM:LED-5MM-POL"	""	""
"D703"	"LED"	"01RetroBrew:LED"	"N8VEM:LED-5MM-POL"	""	""
"D704"	"LED"	"01RetroBrew:LED"	"N8VEM:LED-5MM-POL"	""	""
"K401"	"CONN_3"	"conn:CONN_3"	"pin_array:PIN_ARRAY_3X1"	"Symbole general de connecteur"	""
"K402"	"CONN_3"	"conn:CONN_3"	"pin_array:PIN_ARRAY_3X1"	"Symbole general de connecteur"	""
"K601"	"RESET"	"conn:CONN_3"	"pin_array:PIN_ARRAY_3X1"	"Symbole general de connecteur"	""
"K801"	"CONN_3"	"conn:CONN_3"	"pin_array:PIN_ARRAY_3X1"	"Symbole general de connecteur"	""
"P301"	"C96ABC"	"00N8VEM:C96ABC"	"01N8VEM:C96ABCM-RA"	""	""
"P302"	"CONN_4"	"conn:CONN_4"	"01N8VEM:PCpower4"	"Symbole general de connecteur"	""
"P501"	"OSC16MhZ"	"conn:DIL8"	"Kicad:OSC_8DIP"	""	""
"P502"	"CONN_17X2"	"SBC-188:CONN_17X2"	"01N8VEM:SHROUDED_17X2"	""	""
"P601"	"CONN_3"	"conn:CONN_3"	"pin_array:PIN_ARRAY_3X1"	"Symbole general de connecteur"	""
"P701"	"OSC1.8432Mhz"	"conn:DIL8"	"Kicad:OSC_8DIP"	""	""
"P702"	"CONN_5X2"	"conn:CONN_5X2"	"01N8VEM:SHROUDED_5x2"	"Symbole general de connecteur"	""
"P703"	"CONN_4X2"	"conn:CONN_4X2"	"pin_array:pin_array_4x2"	"Symbole general de connecteur"	""
"P801"	"IDE40-connector"	"01RetroBrew:IDE40-connector"	"Kicad:SHROUDED_20X2"	""	""
"P802"	"IDE40-connector"	"01RetroBrew:IDE40-connector"	"Kicad:SHROUDED_20X2"	""	""
"P803"	"CONN_13X2"	"conn:CONN_13X2"	"Kicad:SHROUDED_13x2"	""	""
"P804"	"CONN_2"	"conn:CONN_2"	"pin_array:PIN_ARRAY_2X1"	"Symbole general de connecteur"	""
"P805"	"CONN_3X2"	"00N8VEM:CONN_3X2"	"pin_array:pin_array_3x2"	""	""
"R401"	"22K"	"device:R"	"discret:R3"	"Resistance"	""
"R601"	"68"	"device:R"	"discret:R3"	"Resistance"	""
"R602"	"10"	"device:R"	"discret:R3"	"Resistance"	""
"R701"	"1K"	"device:R"	"discret:R3"	"Resistance"	""
"RR501"	"1K"	"device:RR9"	"discret:r_pack9"	""	""
"RR601"	"10K"	"device:RR9"	"discret:r_pack9"	""	""
"RR701"	"4.7K"	"00N8VEM:RR4"	"Kicad:r_pack4"	""	""
"RR801"	"10K"	"device:RR9"	"discret:r_pack9"	""	""
"SW601"	"SW_PUSH"	"device:SW_PUSH"	"discret:SW_PUSH_SMALL"	"Push Button"	""
"U101"	"74LS00"	"00N8VEM:74LS00"	"dip_sockets:DIP-14__300"	""	""
"U201"	"80188"	"00N8VEM:80188"	"Kicad:80188"	""	""
"U202"	"OSC_2X"	"conn:DIL8"	"Kicad:OSC_8DIP"	""	""
"U203"	"74ALS373"	"74xx:74LS373"	"dip_sockets:DIP-20__300"	"8 bits Latch, 3 state Out"	""
"U204"	"74ALS373"	"74xx:74LS373"	"dip_sockets:DIP-20__300"	"8 bits Latch, 3 state Out"	""
"U205"	"GAL22V10"	"00N8VEM:GAL22V10"	"dip_sockets:DIP-24__300"	""	""
"U401"	"SRAM_512K"	"00N8VEM:SRAM_512K"	"dip_sockets:DIP-32__600"	""	""
"U402"	"SRAM_512K"	"00N8VEM:SRAM_512K"	"dip_sockets:DIP-32__600"	""	""
"U403"	"29F040"	"00N8VEM:29F040"	"dip_sockets:DIP-32__600"	""	""
"U501"	"WD37C65"	"SBC-188:WD37C65"	"sockets:PLCC44"	""	""
"U502"	"GAL22V10"	"00N8VEM:GAL22V10"	"dip_sockets:DIP-24__300"	""	""
"U601"	"74LS245"	"74xx:74LS245"	"dip_sockets:DIP-20__300"	"Octal BUS Transceivers, 3 State out"	""
"U602"	"74LS245"	"74xx:74LS245"	"dip_sockets:DIP-20__300"	"Octal BUS Transceivers, 3 State out"	""
"U603"	"74LS245"	"74xx:74LS245"	"dip_sockets:DIP-20__300"	"Octal BUS Transceivers, 3 State out"	""
"U604"	"74LS245"	"74xx:74LS245"	"dip_sockets:DIP-20__300"	"Octal BUS Transceivers, 3 State out"	""
"U605"	"74LS244"	"74xx:74LS244"	"dip_sockets:DIP-20__300"	"8 bits Bus Buffer 3 State out"	""
"U606"	"74LS240"	"74xx:74LS240"	"dip_sockets:DIP-20__300"	"8 bits BUS Buffer (Inverter) 3 State out"	""
"U701"	"TL16C550FN"	"00N8VEM:TL16C550FN"	"sockets:PLCC44"	""	""
"U702"	"74LS259"	"74xx:74LS259"	"dip_sockets:DIP-16__300"	"8 bits addressable latch"	""
"U703"	"DS1302"	"special:DS1302"	"dip_sockets:DIP-8__300"	"TimeKeeper DALLAS/MAXIM"	""
"U704"	"74LS05"	"74xx:74LS05"	"dip_sockets:DIP-14__300"	"Inverseur Open Collect"	""
"U706"	"MAX233"	"00N8VEM:MAX233"	"dip_sockets:DIP-20__300"	""	""
"U801"	"82C55-PLCC"	"00N8VEM:8255PLCC"	"sockets:PLCC44"	""	""
"U802"	"74LS04"	"00N8VEM:74LS04"	"dip_sockets:DIP-14__300"	""	""
"X701"	"CRYSTAL"	"device:CRYSTAL"	"Kicad:Tuning_Fork_Header_Straight_1x02_Pitch1.00mm"	""	""
